,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
ZUUW70LA0,UU200W U80A0,U80A,"3,200 x 1",Hermetic Motor Compressor,-,8.00 ~ 20.00 ~ 22.00,-,"1,090 x 1,625 x 380",EEV,-,55 x 2,124 x 2,BLDC,Propeller,-,10.00 ~ 23.00~ 25.30,ZUUW70LA0,131.0,-,7/8,22.22,1/2,12.7,2.19 ~ 6.06 ~ 7.59,2.05 ~ 5.70 ~ 7.05,"3, 380-415, 50",5C x 2.5,4950,22.22,12.7,R32,9.41,8.85,77,77,62,64,-15~48,-,-18~18,-,Single CAC ODU
ZUUW85LA0,UU250W U80A0,U80A,"5,300 x 1",Hermetic Motor Compressor,-,9.20 ~ 23.00 ~ 25.30,-,"1,090 x 1,625 x 380",EEV,-,55 x 2,250 x 2,BLDC,Propeller,-,10.80 ~ 25.00~ 27.50,ZUUW85LA0,131.0,-,7/8,22.22,1/2,12.7,2.85 ~ 7.93 ~ 9.12,2.37 ~ 6.59 ~ 7.80,"3, 380-415, 50",5C x 2.5,4950,22.22,12.7,R32,12.3,10.2,77,77,62,64,-15~48,-,-18~18,-,Single CAC ODU
