,Chassis name##other##,Type##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Current_Current(MAX)_A##other##,Cooling Operation Range(Leaving Water)_For Fan Coil Unit(Min ~ Max)##other##,Cooling Operation Range(Leaving Water)_For under floor(Min ~ Max)##other##,Heating Operation Range(Leaving Water)_Space Heating(Min ~ Max)##other##,Heating Operation Range(Leaving Water)_Domestic Hot Water(Min ~ Max)##other##,Main water pump Type##other##,Main water pump Model##other##,Main water pump Motor type##other##,Main water pump Steps of Pump Performance##other##,Main water pump Power input (W)##other##,Main water pump Max Head (m)##other##,Expansion Tank Volume(Max) (L)##other##,Expansion Tank Water Pressure(Max) (bar)##other##,Expansion Tank Water Pressure(Pre-charged) (bar)##other##,Strainer Mesh size (mesh)##other##,Strainer Max. particle size (mm)##other##,Strainer Material##other##,Safety Valve Pressure Limit (bar)##other##,DHW Safety valve Pressure Limit (bar)##other##,3 Way Model (Maker Name)##other##,3 Way Valve Motor Type##other##,3 Way Valve Flow coefficient##other##,Flow Sensor Type##other##,Flow Sensor Model##other##,Flow Sensor Measuring range (L/min)##other##,Water Pressure sensor Model##other##,Water Pressure sensor Measuring Range (Bar (G))##other##,DHW Tank Type##other##,DHW Tank Water Volume (L)##other##,DHW Tank Material##other##,DHW Tank Internal Thermal Protect limit (C)##other##,DHW Tank Rated pressure (Pressure limit) (bar)##other##,DHW Tank Insulation Material##other##,DHW Tank Insulation Thickness (mm)##other##,Electric Backup Heater_Type##other##,Electric Backup Heater_Power Supply (V_Ph_Hz)##other##,Electric Backup Heater_Number of Heating Coil##other##,Electric Backup Heater_Capacity Combination(KW)##other##,Electric Backup Heater_Rated Current(A)##other##,Electric Backup Heater_Maximum Electrical Power(KW)##other##,Electric Backup Heater_Power Supply Cable(H07RN-F)##other##,Heat Exchanger (Water - DHW) Type##other##,Heat Exchanger (Water - DHW) Quantity##other##,Heat Exchanger (Water - DHW) Surface area(mm2)##other##,Heat Exchanger (Refrigerant to Water) Type##other##,Heat Exchanger (Refrigerant to Water) Quantity##other##,Heat Exchanger (Refrigerant to Water) Number of Plate##other##,Refrigerant Piping Connection_Liquid_mm(inch)##other##,Refrigerant Piping Connection_Gas_mm(inch)##other##,Refrigerant Piping Connection_Connection Type(Liquid)##other##,Refrigerant Piping Connection_Connection Type(Gas)##other##,Piping Connections Water Circuit Inlet (mm(inch))##other##,Piping Connections Water Circuit Outlet (mm(inch))##other##,Piping Connections DHW Tank Water Circuit Cold Inlet (mm(inch))##other##,Piping Connections DHW Tank Water Circuit Hot Outlet (mm(inch))##other##,Piping Connections DHW Tank Water Circuit Reciculation (mm(inch))##other##,Sound Power Level_Heating(Rated) (dB(A))##other##,Dimensions Unit (W x H x D) (mm)##other##,Dimensions Shipping (W x H x D) (mm)##other##,Weight  Unit (kg)##other##,Weight  Shipping (kg)##other##,Exterior Color##other##,Exterior RAL Code##other##,Wiring Connections Power and Communication Cable (mm2xcores)##other##
FHNW20606Y0,K5,Combi Unit,HN1616HY NK0,FHNW20606Y0,0.6,5 ~ 27,16 ~ 27,15 ~ 75,15 ~ 80,-,-,-,-,-,-,8,3,1,-,-,-,-,10,Sanhua QSF-A02M20,2-2 Step motor(DC 12V),12,-,-,-,-,-,"Internal coil type integrated hotwater tank",200,Duplex 2205,85,10,Polyurethane foam,50,Sheath,"220-240, 1, 50",2,3.0 + 3.0,26,6,4.0 x 3C,Coil Heat Exchanger,1,1.81,-,-,-,-,-,-,-,FemaleG1 according to ISO228-1(parallel pipe threads),FemaleG1 according to ISO228-1(parallel pipe threads),FemaleG1 according to ISO228-1(parallel pipe threads),FemaleG1 according to ISO228-1(parallel pipe threads),FemaleG1 according to ISO228-1(parallel pipe threads),39,"600 x 1,750 x 660","660 x 2,009 x 750",108,127,Noble White,RAL 9016,0.75 x 3C / 0.75 x 2C
FHNW20809Y0,K5,Combi Unit,HN1639HY NK0,FHNW20809Y0,0.6,5 ~ 27,16 ~ 27,15 ~ 75,15 ~ 80,-,-,-,-,-,-,8,3,1,-,-,-,-,10,Sanhua QSF-A02M21,2-2 Step motor(DC 12V),12,-,-,-,-,-,"Internal coil type integrated hotwater tank",200,Duplex 2205,85,10,Polyurethane foam,50,Sheath,"380-415, 3, 50",3,3.0 + 3.0 + 3.0,13,9,2.5 x 4C,Coil Heat Exchanger,1,1.81,-,-,-,-,-,-,-,FemaleG1 according to ISO228-1(parallel pipe threads),FemaleG1 according to ISO228-1(parallel pipe threads),FemaleG1 according to ISO228-1(parallel pipe threads),FemaleG1 according to ISO228-1(parallel pipe threads),FemaleG1 according to ISO228-1(parallel pipe threads),39,"600 x 1,750 x 660","660 x 2,009 x 750",108,127,Noble White,RAL 9016,0.75 x 3C / 0.75 x 2C
