,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##,Water Inlet Connection Diameter##pipe_size##Millimeters,Water Outlet Connection Diameter##pipe_size##Millimeters
FHBW076B0,UN36B,0.75 x 2C,Hermetic Motor Compressor,-,5.0,-,"1,320 x 1,019 x 520",-,62 x 1,0.124 x 1,Propeller,-,7,-,FHBW076B0 [HM071HF UB40],130,-,1.14,1.40,"1, 220-240, 50",0.9,-,R290,-,27,5~48,-,-28~35,-,AWHP Monobloc,25.4,25.4
FHBW096B0,UN36B,0.75 x 2C,Hermetic Motor Compressor,-,5.5,-,"1,320 x 1,019 x 520",-,68 x 1,0.124 x 1,Propeller,-,9,-,FHBW096B0 [HM091HF UB40],130,-,1.31,1.91,"1, 220-240, 50",0.9,-,R290,-,28,5~48,-,-28~35,-,AWHP Monobloc,25.4,25.4
FHBW098B0,UN36B,0.75 x 2C,Hermetic Motor Compressor,-,5.5,-,"1,320 x 1,019 x 520",-,68 x 1,0.124 x 1,Propeller,-,9,-,FHBW098B0 [HM093HF UB40],130,-,1.31,1.91,"3, 380-415, 50",0.9,-,R290,-,28,5~48,-,-28~35,-,AWHP Monobloc,25.4,25.4
