,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##,Water Inlet Connection Diameter##pipe_size##Millimeters,Water Outlet Connection Diameter##pipe_size##Millimeters
ZHBW518A0,UXC,1.0 - 1.5 x 2C,Hermetically Sealed Scroll,-,51.0,-,"1,640 x 1,690 x 825",-,430,1.5 x 2,Propeller,-,51.0,,ZHBW518A0 [HM513MR UXC0],335,-,11.33,11.86,"3, 380-415, 50",10,-,R32,58,54,10 ~ 48,-,-25 ~ 35,-,AWHP Monobloc Big R32,38.1,38.1
