,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZBNW70GB8A0,UB200 N80,"2,472 / 2,542 / 2,260",70.0 / 65.0 / 60.0,B8,32,68240,20,61-1/2 x 18-1/8 x 27-3/32,"1,562 x 460 x 688",375 x 2,BLDC,Sirocco Fan,78480,23000,ZBNW70GB8A0,87,-,1-1/4,32.0,7/8,22.2 ,1/2,12.7 ,4C x 1.0 (16),-,-,"1, 220-240, 50",22.2,12.7,R32,5.4,77,45 / 43 / 42,-,High Static Duct
ZBNW85GB8A0,UB250 N80,"2,825 / 2,542 / 2,260",80.0 / 72.0 / 64.0,B8,32,78480,23,61-1/2 x 18-1/8 x 27-3/32,"1,562 x 460 x 688",375 x 2,BLDC,Sirocco Fan,85300,25000,ZBNW85GB8A0,87,-,1-1/4,32.0,7/8,22.2 ,1/2,12.7 ,4C x 1.0 (16),-,-,"1, 220-240, 50",22.2,12.7,R32,5.4,77,45 / 43 / 42,-,High Static Duct
