,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZTNW36GYLA0,UT36F NY0,-,25.0 / 21.0 / 19.0,TY,32,-,11,-,1050 x 330 x 1050,136 x 1,BLDC,3D Turbo Fan,-,12.2,ZTNW36GYLA0,30,66.1,-,32,5/8,15.88,3/8,9.52,4C x 0.75,90 / 66 / 48,-,"1,220-240,50 / 1,220,60",15.88,9.52,R32,0.70 / 0.60 / 0.40,59,44.0 / 40.0 / 38.0,47.0 / 43.0 / 40.0,Round Cassette
ZTNW48GYLA0,UT48F NY0,-,29.0 / 25.0 / 21.0,TY,32,-,13.4,-,1050 x 330 x 1050,136 x 1,BLDC,3D Turbo Fan,-,15.5,ZTNW48GYLA0,30,66.1,-,32,5/8,15.88,3/8,9.52,4C x 0.75,125 / 90 / 66,-,"1,220-240,50 / 1,220,60",15.88,9.52,R32,0.80 / 0.70 / 0.60,60,47.0 / 44.0 / 40.0,49.0 / 46.0 / 42.0,Round Cassette
