,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZTNW24GBLA1,CT24F NB0,-,17.0 / 15.0 / 13.0,TP-B,32,-,6.8,33-1/16 x 9-29/64 x 33-1/16,840 x 204 x 840,50.25 x 1,BLDC,3D Turbo Fan,-,7.5,ZTNW24GBLA1,21.1,46.5,1-1/4,32.0,5/8,15.88,3/8,9.52,4C x 0.75,36 / 26 / 21,-,"1/220-240/50, 1/220/60",15.88,9.52,R32,0.50 / 0.46 / 0.44,53,38 / 36 / 34,38 / 36 / 34,4way CST(Dual Vane)
ZTNW30GBLA1,UT30F NB0,-,19.0 / 17.0 / 15.5,TP-B,32,-,8,33-1/16 x 9-29/64 x 33-1/16,840 x 204 x 840,50.25 x 1,BLDC,3D Turbo Fan,-,8.9,ZTNW30GBLA1,21.1,46.5,1-1/4,32.0,5/8,15.88,3/8,9.52,4C x 0.75,40 / 33 / 26,-,"1/220-240/50, 1/220/60",15.88,9.52,R32,0.52 / 0.49 / 0.46,57,40.0 / 37.0 / 35.0,40.0 / 37.0 / 35.0,4way CST(Dual Vane)
