,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZVNW24GM2H1,UV24FH N20,-,23 / 21 / 19,VM2,32,-,2.70 ~ 6.80 ~ 8.30,-,"1,600 x 235 x 690",125 x 1,BLDC,Cross flow Fan,-,3.00 ~ 7.50 ~ 9.40,ZVNW24GM2H1,37.4,82.4,-,32,5/8,15.88,3/8,9.52,4C x 0.75,35 / 32 / 27,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.54 / 0.52 / 0.49,60,43 / 42 / 40,43 / 42 / 40,Ceiling Suspended
ZVNW30GM2H1,UV30FH N20,-,23 / 21 / 19,VM2,32,-,3.20 ~ 8.00 ~ 9.50,-,"1,600 x 235 x 690",125 x 1,BLDC,Cross flow Fan,-,3.60 ~ 8.90 ~ 10.60,ZVNW30GM2H1,37.4,82.4,-,32,5/8,15.88,3/8,9.52,4C x 0.75,35 / 32 / 27,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.54 / 0.52 / 0.49,60,43 / 42 / 40,43 / 42 / 40,Ceiling Suspended
ZVNW36GM2H1,UV36FH N20,-,30 / 25 / 20,VM2,32,-,3.80 ~ 9.50 ~ 12.80,-,"1,600 x 235 x 690",125 x 1,BLDC,Cross Flow Fan,-,4.30 ~ 10.80 ~ 13.70,ZVNW36GM2H1,37.4,82.4,-,32,5/8,15.88,3/8,9.52,4C x 0.75,59 / 40 / 28,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.62 / 0.56 / 0.50,62,48 / 44 / 40,48 / 44 / 40,Ceiling Suspended
ZVNW42GM2H1,UV42FH N20,-,30 / 25 / 20,VM2,32,-,4.80 ~ 12.10 ~ 14.50,-,"1,600 x 235 x 690",125 x 1,BLDC,Cross Flow Fan,-,5.40 ~ 13.50 ~ 16.20,ZVNW42GM2H1,37.4,82.4,-,32,5/8,15.88,3/8,9.52,4C x 0.75,59 / 40 / 28,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.62 / 0.56 / 0.50,62,48 / 44 / 40,48 / 44 / 40,Ceiling Suspended
