,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
ZUUW48GA1,UUD1 U30,U3,"3,200 x 1",LG Inverter Scroll,18425 ~ 45722 ~ 53502,5.40 ~ 13.40 ~ 15.68,37-13/32 x 54-21/64 x 12-63/64,"950 x 1,380 x 330",Electronic Expansion Valve,1942 x 2,55 x 2,124 x 2,BLDC,Propeller,21155 ~ 52888 ~ 59780,6.20 ~ 15.50 ~ 17.52,ZUUW48GA1,85,187,5/8,15.88 ,3/8,9.52,0.90 ~ 4.50 ~ 5.85,0.90 ~ 4.77 ~ 5.82,"1, 220-240, 50",3C x 6.0,3000,15.88 ,9.52,R32,19.70,20.60,69,69,52,53,-15 ~ 48,5 ~ 118.4,-20 ~ 18,-4 ~ 64.4,SingleCAC_Free_Combi
ZUUW48LA1,UUD3 U30,U3,"3,200 x 1",LG Inverter Scroll,18425 ~ 45722 ~ 53502,5.40 ~ 13.40 ~ 15.68,37-13/32 x 54-21/64 x 12-63/64,"950 x 1,380 x 330",Electronic Expansion Valve,1942 x 2,55 x 2,124 x 2,BLDC,Propeller,21155 ~ 52888 ~ 59780,6.20 ~ 15.50 ~ 17.52,ZUUW48LA1,85,187,5/8,15.88 ,3/8,9.52,0.90 ~ 4.50 ~ 5.85,0.90 ~ 4.77 ~ 5.82,"3, 380-415, 50",5C x 2.5,3000,15.88 ,9.52,R32,7.00,7.30,69,69,52,53,-15 ~ 48,5 ~ 118.4,-20 ~ 18,-4 ~ 64.4,SingleCAC_Free_Combi
