,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZTNW18GBLH1,UT18FH NB0,600 / 547 / 494,17.0 / 15.5 / 14.0,TP-B,32,6824 ~ 17061 ~ 20473,2.00 ~ 5.00 ~ 6.00,33-1/16 x 9-29/64 x 33-1/16,840 x 204 x 840,50.25 x 1,BLDC,3D Turbo Fan,7848 ~ 19790 ~ 23885,2.30 ~ 5.80 ~ 7.00,ZTNW18GBLH1 ,21.1,46.5,1-1/4,32.0,1/2,12.7,1/4,6.35,4C x 0.75,33 / 26 / 22,-,"1/220-240/50, 1/220/60",12.7,6.35,R32,0.49 / 0.46 / 0.44,52,37 / 36 / 34,37 / 36 / 34,4way CST(Dual Vane)