,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZVNW18GM1H1,UV18FH N10,-,13 / 12 / 11,VM1,32,-,2.00 ~ 5.00 ~ 6.00,-,"1,200 x 235 x 690",85.9 x 1,BLDC,Cross flow Fan,-,2.30 ~ 5.80 ~ 7.00,ZVNW18GM1H1,27.3,60.2,-,32,1/2,12.7,1/4,6.35,4C x 0.75,17 / 15 / 13,-,"1, 220-240, 50 / 1, 220, 60",12.7,6.35,R32,0.55 / 0.54 / 0.53,55,42 / 40 / 39,42 / 40 / 39,Ceiling Suspended