,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZBNW36GM2A1,UM36F N20,-,32 / 28 / 24,M2,32,-,3.80 ~ 9.50 ~ 12.54,-,"1,250 x 270 x 700",350 x 1,BLDC,Sirocco Fan,-,4.30 ~ 10.80 ~ 13.39,ZBNW36GM2A1,38.5,-,-,25.4 / 32 (using drain pump),5/8,15.88,3/8,9.52,4C x 0.75,183 / 134 / 101,-,"1/220-240/50,1/220/60",15.88,9.52,R32,0.79 / 0.58 / 0.43,60,36 / 34 / 33,36 / 34 / 33,Mid static duct
ZBNW42GM2A1,UM42F N20,-,38 / 33 / 28,M2,32,-,4.80 ~ 12.00 ~ 14.04,-,"1,250 x 270 x 700",350 x 1,BLDC,Sirocco Fan,-,5.40 ~ 13.50 ~ 15.80,ZBNW42GM2A1,38.5,-,-,25.4 / 32 (using drain pump),5/8,15.88,3/8,9.52,4C x 0.75,266 / 200 / 145,-,"1/220-240/50,1/220/60",15.88,9.52,R32,1.15 / 0.86 / 0.63,62,36 / 34 / 33,36 / 34 / 33,Mid static duct

