,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZBNW36GM3H1,UM36FH N30,-,40 / 34 / 28,M3,32,-,3.80 ~ 9.50 ~ 12.80,-,"1,250 x 360 x 700",400 x 1,BLDC,Sirocco Fan,-,4.30 ~ 10.80 ~ 13.70,ZBNW36GM3H1,44.3,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,242 / 159 / 124,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,1.05 / 0.69 / 0.53,65,39 / 38 / 36,39 / 38 / 36,Duct Mid Static
ZBNW42GM3H1,UM42FH N30,-,40 / 34 / 28,M3,32,-,4.80 ~ 12.00 ~ 14.40,-,"1,250 x 360 x 700",400 x 1,BLDC,Sirocco Fan,-,5.40 ~ 13.50 ~ 16.20,ZBNW42GM3H1,44.3,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,242 / 159 / 124,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,1.05 / 0.69 / 0.53,65,39 / 38 / 36,39 / 38 / 36,Duct Mid Static
ZBNW48GM3H1,UM48FH N30,-,40 / 34 / 28,M3,32,-,5.40 ~ 13.40 ~ 16.10,-,"1,250 x 360 x 700",400 x 1,BLDC,Sirocco Fan,-,6.20 ~ 15.50 ~ 17.80,ZBNW48GM3H1,44.3,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,242 / 159 / 124,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,1.05 / 0.69 / 0.53,65,39 / 38 / 36,39 / 38 / 36,Duct Mid Static
