,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZVNW36GM2A1,UV36F N20,-,28 / 24 / 20,VM2,25,-,3.80 ~ 9.50 ~ 12.54,-,"1,600 x 235 x 690",125 x 1,BLDC,Cross Flow Fan,-,4.30 ~ 10.80 ~ 13.39,ZVNW36GM2A1,36.7,80.9,-,25,5/8,15.88,3/8,9.52,4C x 0.75,50 / 35 / 28,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.58 / 0.54 / 0.50,62,46 / 43 / 40,46 / 43 / 40,Ceiling Suspended
ZVNW42GM2A1, UV42F N20,-,28 / 24 / 20,VM2,25,-,4.80 ~ 12.10 ~ 14.16,-,"1,600 x 235 x 690",125 x 1,BLDC,Cross Flow Fan,-,5.40 ~ 13.50 ~ 15.80,ZVNW42GM2A1,36.7,80.9,-,25,5/8,15.88,3/8,9.52,4C x 0.75,50 / 35 / 28,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.58 / 0.54 / 0.50,62,46 / 43 / 40,46 / 43 / 40,Ceiling Suspended
ZVNW48GM2A1, UV48F N20,-,28 / 24 / 20,VM2,25,-,5.40 ~ 13.40 ~ 15.68,-,"1,600 x 235 x 690",125 x 1,BLDC,Cross Flow Fan,-,6.20 ~ 15.50 ~ 17.52,ZVNW48GM2A1,36.7,80.9,-,25,5/8,15.88,3/8,9.52,4C x 0.75,50 / 35 / 28,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.58 / 0.54 / 0.50,62,46 / 43 / 40,46 / 43 / 40,Ceiling Suspended
ZVNW60GM2A1, UV60F N20,-,28 / 24 / 20,VM2,25,-,5.80 ~ 14.40 ~ 15.55,-,"1,600 x 235 x 690",125 x 1,BLDC,Cross Flow Fan,-,6.70 ~ 16.80 ~ 18.14,ZVNW60GM2A1,36.7,80.9,-,25,5/8,15.88,3/8,9.52,4C x 0.75,50 / 35 / 28,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.58 / 0.54 / 0.50,62,46 / 43 / 40,46 / 43 / 40,Ceiling Suspended
