,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZBNW48GM3A1,UM48F N30,-,40 / 34 / 28,M3,32,-,5.40 ~ 13.40 ~ 15.68,-,"1,250 × 360 × 700",400 x 1,BLDC,Sirocco Fan,-,6.20 ~ 15.50 ~ 17.52,ZBNW48GM3A1,43.5,-,-,25.4 / 32 (using drain pump),5/8,15.88,3/8,9.52,4C x 0.75,242 / 159 / 124,-,"1/220-240/50,1/220/60",15.88,9.52,R32,1.05 / 0.69 / 0.53,65,39 / 38 / 36,39 / 38 / 36,Mid static duct
ZBNW60GM3A1,UM60F N30,-,50 / 45 / 40,M3,32,-,5.80 ~ 14.60 ~ 15.77,-,"1,250 × 360 × 700",400 x 1,BLDC,Sirocco Fan,-,6.70 ~ 16.80 ~ 18.14,ZBNW60GM3A1,43.5,-,-,25.4 / 32 (using drain pump),5/8,15.88,3/8,9.52,4C x 0.75,342 / 287 / 242,-,"1/220-240/50,1/220/60",15.88,9.52,R32,1.48 / 1.24 / 1.05,66,42 / 40 / 39,42 / 40 / 39,Mid static duct

