,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZQNW09GALA1,UQ09F NA0,300 / 237 / 177,8.5 / 6.7 / 5.0,QA,16.7,-,1.50 ~ 2.60 ~ 3.40,27-9/16 x 23-5/8 x 8-9/32,700 x 600 x 210,48 x 1,BLDC,Turbo Fan,-,1.60 ~ 3.10 ~ 3.90,ZQNW09GALA1 ,16.3,35.9,-,16.7,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),37 / 30 / 25,-,"1, 220-240, 50 / 1, 220, 60",9.52,6.35,R32,0.53 / 0.51 / 0.48,59,38 / 32 / 27,38 / 32 / 27,Console
ZQNW12GALA1,UQ12F NA0,300 / 237 / 177,8.5 / 6.7 / 5.0,QA,16.7,-,1.50 ~ 3.50 ~ 4.00,27-9/16 x 23-5/8 x 8-9/32,700 x 600 x 210,48 x 1,BLDC,Turbo Fan,-,1.60 ~ 4.00 ~ 4.30,ZQNW12GALA1,16.3,35.9,-,16.7,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),37 / 30 / 25,-,"1, 220-240, 50 / 1, 220, 60",9.52,6.35,R32,0.53 / 0.51 / 0.48,59,38 / 32 / 27,38 / 32 / 27,Console
ZQNW18GALA1,UQ18F NA0,357 / 304 / 254,10.1 / 8.6 / 7.2,QA,16.7,-,2.00 ~ 5.00 ~ 5.80,27-9/16 x 23-5/8 x 8-9/32,700 x 600 x 210,48 x 1,BLDC,Turbo Fan,-,2.00 ~ 4.90 ~ 5.40,ZQNW18GALA1,16.3,35.9,-,16.7,43832,12.7 ,1/4,6.35 ,4C x 0.75 (18),44 / 39 / 35,-,"1, 220-240, 50 / 1, 220, 60",12.7,6.35,R32,0.59 / 0.54 / 0.52,60,44 / 39 / 35,49 / 44 / 39,Console
