,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZJNW30GRLA1,US30F NR0,742 / 600 / 459,21.0 / 17.0 / 13.0,SR,16.5,-,3.20 ~ 8.00 ~ 9.00,47-1/4 x 14-3/16 x 10-7/16,"1,200 x 360 x 265",113 x 1,BLDC,Cross Flow Fan,-,3.60 ~ 9.00 ~ 10.00,ZJNW30GRLA1,18.3,40.3,-,16.5,5/8,15.88,3/8,9.52,4C x 0.75 (18),47(H) / 42(M) / 36 (L),-,"1, 220-240, 50",15.88,9.52,R32,0.32(H) / 0.28(M) / 0.25(L),62,46(H) / 42(M) / 38(L),46(H) / 42(M) / 38(L),Wall mounted
ZJNW36GRLA1,US36F NR0,883 / 742 / 600,25.0 / 21.0 / 17.0,SR,16.5,-,3.80 ~ 9.50 ~ 12.54,47-1/4 x 14-3/16 x 10-7/16,"1,200 x 360 x 265",113 x 1,BLDC,Cross Flow Fan,-,4.30 ~ 10.80 ~ 13.39,ZJNW36GRLA1,18.3,40.3,-,16.5,5/8,15.88,3/8,9.52,4C x 0.75 (18),47(H) / 42(M) / 36 (L),-,"1, 220-240, 50",15.88,9.52,R32,0.32(H) / 0.28(M) / 0.25(L),62,51(H) / 46(M) / 42(L),51(H) / 46(M) / 42(L),Wall mounted
