,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZVNW18GM1A1,UV18F N10,-,13.0 / 12.0 / 11.0,VM1,25,-,2.00 ~ 5.00 ~ 5.80,-,"1,200 x 235 x 690",85.9 x 1,BLDC,Cross flow Fan,-,2.30 ~ 5.80 ~ 6.70,ZVNW18GM1A1,27.3,60.2,-,25,1/2,12.7,1/4,6.35,4C x 0.75,17 / 15 / 13,-,"1, 220-240, 50 / 1, 220, 60",12.7,6.35,R32,0.55 / 0.54 / 0.53,55,42 / 40 / 39,42 / 40 / 39,Ceiling Suspended
ZVNW24GM1A1, UV24F N10,-,16.0 / 15.0 / 14.0,VM1,25,-,2.70 ~ 6.80 ~ 7.50,-,"1,200 x 235 x 690",85.9 x 1,BLDC,Cross flow Fan,-,2.90 ~ 7.30 ~ 8.40,ZVNW24GM1A1,28,61.7,-,25,5/8,15.88,3/8,9.52,4C x 0.75,33 / 26 / 19,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.64 / 0.61 / 0.58,61,46 / 45 / 43,46 / 45 / 43,Ceiling Suspended
ZVNW30GM1A1,UV30F N10,-,19.0 / 17.5 / 16.0,VM1,25,-,3.10 ~ 7.70 ~ 8.80,-,"1,200 x 235 x 690",85.9 x 1,BLDC,Cross flow Fan,-,3.40 ~ 8.60 ~ 9.60,ZVNW30GM1A1,28,61.7,-,25,5/8,15.88,3/8,9.52,4C x 0.75,47 / 40 / 33,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R32,0.70 / 0.67 / 0.64,62,46.0 / 44.0 / 43.0,46.0 / 44.0 / 43.0,Ceiling Suspended
