,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
ZUUW12GA1,UUA1 UL0,UL2,"1,500 x 1",Twin Rotary,5118 ~ 11601 ~ 16037,1.5 ~ 3.4 ~ 4.7,30-5/16 x 21-29/64 x 11-11/32,770 x 545 x 288,Electronic Expansion Valve,988.8 x 1,28 x 1,43.0 x 1,BLDC,Propeller,6141 ~ 13648 ~ 16719,1.80 ~ 4.00 ~ 4.90,ZUUW12GA1,33.3,73.4,3/8,9.52,1/4,6.35,0.33 ~ 1.05 ~ 1.84,0.33 ~ 1.08 ~ 1.63,"1, 220-240, 50",3C x 2.5,1000,9.52,6.35,R32,4.7,4.8,65,-,49,52,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_Free_Combi
