,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZBNW12GM1H1,UM12FH N10,-,16.0 / 12.0 / 9.0,M1,32,-,1.60 ~ 3.50 ~ 5.10,-,900 x 270 x 700,136.5 x 1,BLDC,Sirocco Fan,-,1.60 ~ 4.00 ~ 5.80,ZBNW12GM1H1,25.4,-,-,32,3/8,9.52,1/4,6.35 ,4C x 0.75,150 / 130 / 110,-,"1, 220-240, 50 / 1, 220, 60",9.52,6.35 ,R32,0.85 / 0.76 / 0.67,59,34 / 32 / 30,34 / 32 / 30,Duct Mid Static
ZBNW18GM1H1,UM18FH N10,-,17.5 / 16.0 / 14.0,M1,32,-,2.00 ~ 5.00 ~ 6.00,-,900 x 270 x 700,136.5 x 1,BLDC,Sirocco Fan,-,2.30 ~ 5.80 ~ 7.00,ZBNW18GM1H1,27,-,-,32,1/2,12.7 ,3/8,9.52 ,4C x 0.75,180 / 150 / 130,-,"1, 220-240, 50 / 1, 220, 60",12.7 ,9.52 ,R32,0.98 / 0.85 / 0.76,60,35 / 34 / 32,35 / 34 / 32,Duct Mid Static
