,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZTNW09GRLA1,CT09F NR0,300 / 247 / 211,8.5 / 7.0 / 6.0,TR,32,5118 ~ 8530 ~ 10918,1.50 ~ 2.50 ~ 3.20,22-7/16 x 8-7/16 x 22-7/16,570 x 214 x 570,43 x 1,BLDC,3D Turbo Fan,6141 ~ 10918 ~ 12624,1.80 ~ 3.20 ~ 3.70,ZTNW09GRLA1,12.4,27.3,1-1/4,32.0,3/8,9.52 ,1/4,6.35 ,4C x 0.75,26 / 22 / 19,-,1/ 220-240 / 50,9.52,6.35,R32,0.31 / 0.29 / 0.27,52,36 / 33 / 30,36 / 33 / 30,4Way CST
ZTNW12GRLA1,CT12F NR0,335 / 282 / 247,9.5 / 8.0 / 7.0,TR,32,5118 ~ 11601 ~ 15354,1.50 ~ 3.40 ~ 4.50,22-7/16 x 8-7/16 x 22-7/16,570 x 214 x 570,43 x 1,BLDC,3D Turbo Fan,6141 ~ 13989 ~ 17060,1.80 ~ 4.10 ~ 5.00,ZTNW12GRLA1,12.4,27.3,1-1/4,32.0,3/8,9.52 ,1/4,6.35 ,4C x 0.75,28 / 24 / 20,-,1/ 220-240 / 50,9.52,6.35,R32,0.32 / 0.30 / 0.28,52,38 / 35 / 32,38 / 35 / 32,4Way CST