,Model name (Buyer)##other##,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
ZBNW24GM2H1,UM24FH N20,-,28 / 24 / 21,M2,32,-,2.70 ~ 6.80 ~ 8.30,-,1250 x 270 x 700,350 x 1,BLDC,Sirocco Fan,-,3.00 ~ 7.50 ~ 9.40,ZBNW24GM2H1,39.3,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,134 / 101 / 80,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,0.58 / 0.43 / 0.35,59,34 / 33 / 32,34 / 33 / 32,Duct Mid Static
ZBNW30GM2H1,UM30FH N20,-,28 / 24 / 21,M2,32,-,3.10 ~ 7.80 ~ 9.30,-,1250 x 270 x 700,350 x 1,BLDC,Sirocco Fan,-,3.60 ~ 9.00 ~ 10.70,ZBNW30GM2H1,39.3,-,-,32,5/8,15.88 ,3/8,9.52 ,4C x 0.75,134 / 101 / 80,-,"1, 220-240, 50 / 1, 220, 60",15.88 ,9.52 ,R32,0.58 / 0.43 / 0.35,59,34 / 33 / 32,34 / 33 / 32,Duct Mid Static
