,Model name (Buyer)##other##,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
ZUUW30GA1,UUC1 U40,U4,"2,020 x 1",Twin Rotary,9212 ~ 23202 ~ 27297,2.70 ~ 6.80 ~ 8.00,37-13/32 x 32-53/64 x 12-63/64,950 x 834 x 330,Electronic Expansion Valve,2048 x 1,58 x 1,124 x 1,BLDC,Propeller,10236 ~ 25591 ~ 30709,3.00 ~ 7.50 ~ 9.00,ZUUW30GA1,85,187,5/8,15.88 ,3/8,9.52,0.40 ~ 1.95 ~ 2.69,0.50 ~ 2.27 ~ 3.29,"1 , 220-240 , 50",3C x 2.5,1900,15.88 ,9.52,R32,8.7,10.1,65,-,48,52,-15 ~ 48,5 ~ 118.4,-18~ 18,-0.4 ~ 64.4,SingleCAC Standard Inverter