,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AUUW85LAE",U7,"6,800 x 1",Hermetically Sealed Scroll,"31,400 ~ 78,480 ~ 86,330",9.2 ~ 23.0 ~ 25.3,42.9x 64.0 x15.0,"1,090 x 1,625 x 380",Electronic Expansion Valve,2048.33 x 1,58 x 1,250.0 x 2,BLDC,Axial Flow Fan,"36,850 ~ 92,130 ~ 101,350",10.8 ~ 27.0 ~ 29.7,UU85W,AUUW85LAE,144.0 ,317,7/8,22.2,1/2,12.7,8.19,8.31,"3, 380-415, 50",5C x 2.5 (12),"5,500 ",22.2,12.7,R410A,13.5,13.6,74,-,59,60,-20 ~ 48,-4 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_StandardInverter

