,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ABNW70GB9A0","2,472 / 2,542 / 2,260",70.0 / 65.0 / 60.0,B9,32,"25,930~64,830 ~71,310",7.6 ~ 19.0 ~ 20.9,61-17/32 x 18-1/32 x 31-5/32,"1,563 x 458 x 791",375 x 2,BLDC,Sirocco Fan,"30,700 ~ 76,430 ~83,930",9.0 ~ 22.4 ~ 24.6,UB70,ABNW70GB9A0,90,198,1-1/4,32.0,1/1,25.4 ,3/8,9.52 ,4C x 1.0 (16),-,-,"1, 220-240, 50",25.4,9.52,R410A,3,61,43 / 41 / 40,-,Duct (High)
"ABNW85GB9A0","2,825 / 2,542 / 2,260",80.0 / 72.0 / 64.0,B9,32,"31,400 ~ 78,480 ~ 86,330",9.2 ~ 23.0 ~ 25.3,61-17/32 x 18-1/32 x 31-5/32,"1,563 x 458 x 791",375 x 2,BLDC,Sirocco Fan,"36,850 ~ 92,130 ~ 101,350",10.8 ~ 27.0 ~ 29.7,UB85,ABNW85GB9A0,90,198,1-1/4,32.0,7/8,22.2 ,1/2,12.7 ,4C x 1.0 (16),-,-,"1, 220-240, 50",22.2,12.7,R410A,3,61,43 / 41 / 40,-,Duct (High)

