,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ATNH18GQLE2",459 / 424 / 353,13.0 / 12.0 / 11.0,TQ,32,"6,800 ~ 17,100 ~ 18,700",2.00 ~ 5.00 ~ 5.50,22-7/16 x 10-3/32 x 22-7/16,570 x 256 x 570,43 x 1,BLDC,Turbo Fan,"7,500 ~ 19,800 ~ 23,200",2.20 ~ 5.80 ~ 6.80,CT18,ATNH18GQLE2,15.5,34.2,1-1/4,32.0,1/2,12.7 ,1/4,6.35 ,4C x 0.75 (18),10 / 30 / 40,-,"1, 220-240, 50",12.7,6.35,R410A,0.4,55,41 / 39 / 36,-,4Way CST

