,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ABNW48GM3A0","1,412 / 1,200 / 988",40.0 / 34.0 / 28.0,M3,32,"19,100 ~ 47,800 ~ 52,600",5.60 ~ 14.0 ~ 15.4,49-7/32 x 14-3/16 x 27-9/16,"1,250 x 360 x 700",290 x 1,BLDC,Sirocco Fan,"22,500 ~ 53,900 ~ 62,100",6.60 ~ 15.8 ~ 18.2,UM48,ABNW48GM3A0,42.5,93.7,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),180,-,"1, 220-240, 50 / 1, 230, 60",15.88,9.52,R410A,1.1,65,39 / 37 / 35,-,Duct (Mid)
"ABNW60GM3A0","1,765 / 1,589 / 1,412",50.0 / 45.0 / 40.0,M3,32,"20,100 ~ 51,200 ~ 55,600",5.90 ~ 15.0 ~ 16.3,49-7/32 x 14-3/16 x 27-9/16,"1,250 x 360 x 700",290 x 1,BLDC,Sirocco Fan,"23,200 ~ 57,300 ~ 63,800",6.80 ~ 16.8 ~ 18.7,UM60,ABNW60GM3A0,42.5,93.7,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),290,-,"1, 220-240, 50 / 1, 230, 60",15.88,9.52,R410A,1.65,66,42 / 40 / 39,-,Duct (Mid)

