,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"APNH48GTLA0","1,271 / 1,095 / 954 / 812",36.0 / 31.0 / 27.0 / 23.0,PT2,32,"20,500 ~ 45,700 ~ 51,900",6.00 ~ 13.4 ~ 15.2,23-7/32 x 72-7/16 x 18-1/8,"590 x 1,840 x 460",224 x 1,BLDC,Sirocco,"20,500 ~ 52,900 ~ 58,300",6.00 ~ 15.5 ~ 17.1,UP48,APNH48GTLA0,50,110.2,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),150 x 1,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R410A,0.9,59,55 / 52 / 49 / 45,-,Floor Standing

