,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ATNH09GRLE2",300 / 265 / 230,8.5 / 7.0 / 6.0,TR,32,"3,400 ~ 8,500 ~ 9,400",1.00 ~ 2.50 ~ 2.75,22-7/16 x 8-7/16 x 22-7/16,570 x 214 x 570,43 x 1,BLDC,Turbo Fan,"4,100 ~ 10,200 ~ 11,300",1.20 ~ 3.00 ~ 3.30,CT09,ATNH09GRLE2,14,30.9,1-1/4,32.0,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),10 / 20 / 20,-,"1, 220-240, 50",9.52,6.35,R410A,0.4,48,36 / 33 / 30,-,4Way CST
"ATNH12GRLE2",336 / 283 / 230,9.5 / 8.0 / 7.0,TR,32,"4,600 ~ 11,600 ~ 12,800",1.36 ~ 3.40 ~ 3.74,22-7/16 x 8-7/16 x 22-7/16,570 x 214 x 570,43 x 1,BLDC,Turbo Fan,"5,500 ~ 13,600 ~ 15,000",1.60 ~ 4.00 ~ 4.40,CT12,ATNH12GRLE2,14,30.9,1-1/4,32.0,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),10 / 20 / 20,-,"1, 220-240, 50",9.52,6.35,R410A,0.4,51,38 / 35 / 32,-,4Way CST

