,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ATNH24GPLE2",600 / 530 / 459,17.0 / 15.0 / 13.0,TP,32,"9,700 ~ 23,200 ~ 26,600",2.84 ~ 6.80 ~ 7.80,33-1/16 x 8-1/32 x 33-1/16,840 x 204 x 840,60 x 1,BLDC,Turbo Fan,"10,900 ~ 27,300 ~ 30,000",3.20 ~ 8.00 ~ 8.80,CT24,ATNH24GPLE2,20.5,45.2,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),20 / 50 / 60,-,"1, 220-240, 50",15.88,9.52,R410A,0.6,57,38 / 36 / 34,-,4Way CST
"ATNH30GPLE2",671 / 600 / 530,19.0 / 17.0 / 15.0,TP,32,"10,900 ~ 27,300 ~ 30,000",3.20 ~ 8.00 ~ 8.80,33-1/16 x 8-1/32 x 33-1/16,840 x 204 x 840,60 x 1,BLDC,Turbo Fan,"12,300 ~ 30,700 ~ 33,800",3.60 ~ 9.00 ~ 9.90,UT30W ,ATNH30GPLE2,20.5,45.2,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),30 / 70 / 80,-,"1, 220-240, 50",15.88,9.52,R410A,0.6,57,40 / 37 / 35,-,4Way CST

