,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ATNH36GNLE2",848 / 777 / 671,24.0 / 22.0 / 19.0,TN,32,"13,600 ~ 34,100 ~ 37,500",4.00 ~ 10.0 ~ 11.0,33-1/16 x 9-11/16 x 33-1/16,840 x 246 x 840,124 x 1,BLDC,Turbo Fan,"15,000 ~ 37,500 ~ 41,300",4.40 ~ 11.0 ~ 12.1,UT36W ,ATNH36GNLE2,22.3,49.2,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),40 / 130 / 140,-,"1, 220-240, 50",15.88,9.52,R410A,0.6,62,43 / 40 / 37,-,4Way CST

