,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"AJNW30GVLA0",777 / 671 / 565,22.0 / 19.0 / 16.0,SV,21.5,"11,900 ~ 26,600 ~ 29,000",3.50 ~ 7.80 ~ 8.50,46.8 x 13.6 x 10.4,"1,190 x 346 x 265",82.1 x 1,BLDC,Cross Flow Fan,"13,600 ~ 28,700 ~ 31,400",4.00 ~ 8.40 ~ 9.20,UJ30,AJNW30GVLA0,15.7,34.6,27/32,21.5,5/8,15.88 ,3/8,9.52 ,4C x 1.0 (18),50 / 100 / 140,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R410A,- / - / 0.6,61,45 / 42 / 40,-,Wall Mounted
"AJNW36GVLA0",953 / 847 / 706,27.0 / 24.0 / 20.0,SV,21.5,"13,600 ~ 32,400 ~ 35,800",4.00 ~ 9.50 ~ 10.50,46.8 x 13.6 x 10.4,"1,190 x 346 x 265",102.6 x 1,BLDC,Cross Flow Fan,"15,000 ~ 35,800 ~ 39,200",4.40 ~ 10.50 ~ 11.50,UJ36,AJNW36GVLA0,16,35.3,27/32,21.5,5/8,15.88 ,3/8,9.52 ,4C x 1.0 (18),60 / 120 / 160,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R410A,- / - / 0.7,63,48 / 45 / 41,-,Wall Mounted

