,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AUUW186D2",UE,"2,137 x 1",Twin Rotary,"6,800 ~ 16,000 ~ 18,800",2.0 ~ 4.7 ~ 5.5,34-1/4 x 25-25/32 x 12-19/32,870 x 655 x 320,Electronic Expansion Valve,1765.8 x 1,50 x 1,85.4 x 1,BLDC,Propeller,"7,500 ~ 18,800 ~ 20,800",2.2 ~ 5.5 ~ 6.1,UU18W,AUUW186D2,46.0 ,101.4,1/2,12.7,1/4,6.35,1.52,1.58,"1, 220-240, 50",3C x 2.5 (12),"1,400 ",12.7,6.35,R410A,6.6,6.9,60,-,48,51,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_StandardInverter
"AUUW18GAE",UE,"1,500 x 1",Twin Rotary,"6,800 ~ 17,100 ~ 18,700",2.00 ~ 5.00 ~ 5.50,34-1/4 x 25-25/32 x 12-19/,870 x 655 x 320,Electronic Expansion Valve,1765.8 x 1,50 x 1,85.4 x 1,BLDC,Axial,"7,500 ~ 19,800 ~ 23,200",2.20 ~ 5.80 ~ 6.80,-,AUUW18GAE,44.6 ,98.3,1/2,12.7,1/4,6.35,1.56,1.66,"1, 220-240, 50",3C x 2.5 (12),"1,300 ",12.7,6.35,R410A,7.1,7.5,63,-,47,52,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_StandardInverter