,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ABNH09GL1A2",318 / 247 / 194,9.0 / 7.0 / 5.5,L1,32,"3,800 ~ 8,500 ~ 10,900",1.10 ~ 2.50 ~ 3.20,27-9/16 x 7-15/32 x 27-9/16,700 x 190 x 700,19 x 1,BLDC,Sirocco,"4,100 ~ 10,900 ~ 12,300",1.20 ~ 3.20 ~ 3.60,CB09L,ABNH09GL1A2,17.5,38.6,1-1/4,32.0,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),50,-,"1, 220-240, 50 / 1, 220, 60",9.52,6.35,R410A,0.4,49,30 / 26 / 23,-,Duct (Low)

