,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ABNW36GM2A0","1,130 / 988 / 847",32.0 / 28.0 / 24.0,M2,32,"13,600 ~ 34,100 ~ 37,500",4.00 ~ 10.0 ~ 11.0,49-7/32 x 10-5/8 x 27-9/16,"1,250 x 270 x 700",295 x 1,BLDC,Sirocco Fan,"15,400 ~ 38,200 ~ 42,000",4.50 ~ 11.2 ~ 12.3,UM36,ABNW36GM2A0,36,79.4,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),210,-,"1, 220-240, 50 / 1, 230, 60",15.88,9.52,R410A,1.3,60,36 / 34 / 33,-,Duct (Mid)
"ABNW42GM2A0","1,341 / 1,165 / 988",38.0 / 33.0 / 28.0,M2,32,"17,100 ~ 41,300 ~ 45,000",5.00 ~ 12.1 ~ 13.2,49-7/32 x 10-5/8 x 27-9/16,"1,250 x 270 x 700",295 x 1,BLDC,Sirocco Fan,"19,100 ~ 47,800 ~ 51,200",5.60 ~ 14.0 ~ 15.0,UM42,ABNW42GM2A0,37,81.6,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),260,-,"1, 220-240, 50 / 1, 230, 60",15.88,9.52,R410A,1.5,62,38 / 36 / 34,-,Duct (Mid)

