,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"AVNH09GELA2",268 / 244 / 219,7.6 / 6.9 / 6.2,VE,21.5,"3,400 ~ 8,500 ~ 9,400",1.00 ~ 2.50 ~ 2.75,35-7/16 x 19-9/32 x 7-7/8,900 x 490 x 200,20 x 1,BLDC,Cross Flow Fan,"4,100 ~ 10,200 ~ 11,300",1.20 ~ 3.00 ~ 3.30,CV09,AVNH09GELA2,13.7,30.2,27/32,21.5,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),10 / 30,-,"1, 220-240, 50 / 1, 230, 60",9.52,6.35,R410A,0.4,52,38 / 35 / 32,-,Convertible
"AVNH12GELA2",325 / 268 / 219,9.2 / 7.6 / 6.6,VE,21.5,"4,500 ~ 11,300 ~ 12,400",1.32 ~ 3.30 ~ 3.63,35-7/16 x 19-9/32 x 7-7/8,900 x 490 x 200,20 x 1,BLDC,Cross Flow Fan,"5,200 ~ 13,000 ~ 14,300",1.52 ~ 3.80 ~ 4.18,CV12,AVNH12GELA2,13.7,30.2,27/32,21.5,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),20 / 40,-,"1, 220-240, 50 / 1, 230, 60",9.52,6.35,R410A,0.4,56,40 / 36 / 31,-,Convertible

