,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ABNH24GL3A2",706 / 565 / 424,20.0 / 16.0 / 12.0,L3,32,"13,600 ~ 24,200 ~ 26,300",4.00 ~ 7.10 ~ 7.70,43-5/16 x 7-15/32 x 27-9/16,"1,100 x 190 x 700",19 x 2,BLDC,Sirocco,"6,800 ~ 25,600 ~ 28,100",2.00 ~ 7.50 ~ 8.25,CB24L,ABNH24GL3A2,27,59.5,1-1/4,32.0,5/8,15.88 ,3/8,9.52 ,4C x 0.75 (18),150,-,"1, 220-240, 50 / 1, 220, 60",15.88,9.52,R410A,1,58,39 / 35 / 32,-,Duct (Low)

