,Air Flow Rate (H/M/L)(CFM)##other##,Air Flow Rate (H/M/L)(CMM)##other##,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power and Communication Cable##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Power Level (dB(A))##other##,Sound Pressure Level Cooling(dB)##other##,Sound Pressure Level Heating(dB)##other##,Type##other##
"ABNH12GL2A2",353 / 300 / 247,10.0 / 8.5 / 7.0,L2,32,"4,800 ~ 11,600 ~ 12,600",1.40 ~ 3.40 ~ 3.70,35-7/16 x 7-15/32 x 27-9/16,900 x 190 x 700,19 x 1 + 5 x 1,BLDC,Sirocco,"5,500 ~ 13,600 ~ 15,400",1.60 ~ 4.00 ~ 4.50,CB12L,ABNH12GL2A2,23,50.7,1-1/4,32.0,3/8,9.52 ,1/4,6.35 ,4C x 0.75 (18),95,-,"1, 220-240, 50 / 1, 220, 60",9.52,6.35,R410A,0.8,52,31 / 28 / 27,-,Duct (Low)
"ABNH18GL2A2",530 / 441 / 353,15.0 / 12.5 / 10.0,L2,32,"6,800 ~ 17,100 ~ 20,500",2.00 ~ 5.00 ~ 6.00,35-7/16 x 7-15/32 x 27-9/16,900 x 190 x 700,19 x 1 + 5 x 1,BLDC,Sirocco,"7,500 ~ 20,500 ~ 24,600",2.20 ~ 6.00 ~ 7.20,CB18L,ABNH18GL2A2,23,50.7,1-1/4,32.0,1/2,12.7 ,1/4,6.35 ,4C x 0.75 (18),120,-,"1, 220-240, 50 / 1, 220, 60",12.7,6.35,R410A,0.8,54,36 / 34 / 31,-,Duct (Low)

