,Chassis name##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable##other##,Refrigerant Charge (g)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (Cooling)(A)##other##,Running Current (Heating)(A)##other##,Sound Power Level Cooling (dB(A))##other##,Sound Power Level Heating (dB(A))##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AUUW366D2",OU4,"4,000 x 1",Twin Rotary,"13,600 ~ 34,100 ~ 37,500",4.00 ~ 10.0 ~ 11.0,37-13/32 x 46-1/16 x 13,"950 x 1,170 x 330",Electronic Expansion Valve,1589.22 x 2,45 x 2,85.4 x 2,BLDC,Propeller,"15,000 ~ 37,500 ~ 41,300",4.40 ~ 11.0 ~ 12.1,UU36W,AUUW366D2,81.0 ,178.6,5/8,15.88,3/8,9.52,2.82,3.09,"1, 220-240, 50",3C x 5.0 (8),"2,800 ",15.88,9.52,R410A,12.3,13.4,66,-,53,54,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_StandardInverter
"AUUW368D2",OU4,"4,000 x 1",Twin Rotary,"13,600 ~ 34,100 ~ 37,500",4.00 ~ 10.0 ~ 11.0,37-13/32 x 46-1/16 x 13,"950 x 1,170 x 330",Electronic Expansion Valve,1589.22 x 2,45 x 2,85.4 x 2,BLDC,Propeller,"15,000 ~ 37,500 ~ 41,300",4.40 ~ 11.0 ~ 12.1,UU37W,AUUW368D2,85.0 ,187.4,5/8,15.88,3/8,9.52,2.82,3.09,"3, 380-415, 50",5C x 2.5 (12),"2,800 ",15.88,9.52,R410A,4.1,4.4,66,-,53,54,-15 ~ 48,5 ~ 118.4,-18 ~ 18,-0.4 ~ 64.4,SingleCAC_StandardInverter

