,Buyer Model##other##,Factory Model##other##,Capacity_Volume_L##other##,Energy_UEF##other##,Energy_FHR_Gallon/hour##other##,Power Input_Upper Element_W##other##,Power Input_Lower Element_W##other##,Annual Energy Consumption(AEC) (15C / 7C)_kWH##other##,Power Supply_ик_V_Hz##other##,Available Voltage Range_V##other##,Indoor_Air Flow Rate_m3/min##other##,Indoor_Air Flow Rate_CFM##other##,Indoor_Sound Pressure Level_dB(A)##other##,Indoor_Sound Power Level_dB(A)##other##,Indoor_Dimensions_Net (W x H x D)_mm##other##,Indoor_Dimensions_Net (W x H x D)_in##other##,Indoor_Weight_Net_kg##other##,Indoor_Weight_Net_lb##other##,Indoor_Heat Pump Operation Range_C(DB)##other##,Indoor_Heat Pump Operation Range_F(DB)##other##,Indoor_Max. Fuse Size_A##other##,Indoor_Exterior Color Code##other##,Compressor_Type##other##,Compressor_Manufacturer##other##,Max Working Pressure (Water Tank)_kPa##other##,Max Working Pressure (Water Tank)_PSI##other##,Circuit Breaker_A##other##,Power Supply Cable_No.##other##,Power Supply Cable_AWG##other##,Drain Hose Size_I.D_mm##other##,Drain Hose Size_I.D_in##other##,Refrigerant_Type##other##,Refrigerant_Pre Charge_g##other##,Refrigerant_Pre Charge_oz##other##,Refrigerant_Pre Charge_t-Co2 eq##other##,Refrigerant_GWP##other##,Defrost Method##other##,Anode##other##,Foam Insulation_mm##other##,Water Connection Size_inch##other##
R6TS20C-EA0,WH20ESF0.CA,R6TS20C-EA0,200,-,-,2000,-,770/-,"1,230,50",195~265,4.5,-,38,- / 53.0(Indoor),"600 x 1,708 x 608",-,92,-,-7 ~ 43,-,-,RAL 9003,Constant speed rotary,-,1000,-,16,1.5 x 3C,-,19,-,R290,150,-,0.00045,3,Reverse Cycle,ICCP,50,3/4
