,Circuit Breaker (A)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (kW)##other##,Cooling Capacity (Btu/h)##other##,Dimensions (WxHxD)(mm)##other##,Dimensions (WxHxD)(inch)##other##,Efficiency (Cooling)##other##,Efficiency (Heating)##other##,Evaporator Flow rate (Cooling)(LPM)##other##,Evaporator Flow rate (Heating)(LPM)##other##,Evaporator Head Loss (kPa)##other##,Evaporator Type##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CMM)##other##,Fan Air Flow Rate (CFM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Heating Capacity (kW)##other##,Heating Capacity (Btu/h)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Operating Current (A)##other##,Piping Connections Inlet (mm)##other##,Piping Connections Outlet (mm)##other##,Piping Connections Inlet (inch)##other##,Piping Connections Outlet (inch)##other##,Power Communication Cable##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling/Heating (dB(A))##other##
KCHH050LDGC,175,-,Inverter Scroll,171,-,"2,291x2,210x2154",-,3.10,3.60,491,518,18.7,Plate,EEV,-,-,1500 x 6,BLDC,180,-,1422,-,-,65A,65A,-,-,-,55.2,50,"3, 380~415, 50",4.7 x 6,-,R32,68
KCHH060LDGC,175,-,Inverter Scroll,195,-,"2,291x2,210x2154",-,3.00,3.50,558,600,21.5,Plate,EEV,-,-,1500 x 6,BLDC,210,-,1422,-,-,65A,65A,-,-,-,65,60,"3, 380~415, 50",4.7 x 6,-,R32,68
KCHH067LDGC,175,-,Inverter Scroll,222,-,"2,291x2,210x2154",-,2.80,3.40,633,705,28.7,Plate,EEV,-,-,1500 x 6,BLDC,246,-,1422,-,-,65A,65A,-,-,-,79.3,72.4,"3, 380~415, 50",4.7 x 6,-,R32,68
