,Normal Capacity (CMH)##other##,Normal Capacity (CFM)##other##,Power Supply (Ph_V_Hz)##other##,ERV Mode Current (SH/H/L)(A)##other##,ERV Mode Power Input (SH/H/L)(W)##other##,ERV Mode Air Flow (SH/H/L)(CMH)##other##,ERV Mode Air Flow (SH/H/L)(CFM)##other##,ERV Mode External static pressure (SH/H/L)(Pa)##other##,ERV Mode Temperature exchange efficiency (SH/H/L)(%)##other##,ERV Mode Enthalpy exchange efficiency Heating (SH/H/L)(%)##other##,ERV Mode Enthalpy exchange efficiency Cooling (SH/H/L)(%)##other##,ERV Mode Energy Label (A+ to G Scale)##other##,ERV Mode Sound pressure level (SH/H/L)(dB(A))##other##,ERV Mode Sound power level (SH/H/L)(dB(A))##other##,Bypass Mode Current (SH/H/L)(A)##other##,Bypass Mode Power Input (SH/H/L)(W)##other##,Bypass Mode Air Flow (SH/H/L)(CMH)##other##,Bypass Mode Air Flow (SH/H/L)(CFM)##other##,Bypass Mode External static pressure (SH/H/L)(Pa)##other##,Bypass Mode Sound pressure level (SH/H/L)(dB(A))##other##,Heat Exchanger type##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Dimensions (WxHxD)(mm)##other##,Dimensions (WxHxD)(inch)##other##,Duct work Qty(EA)##other##,Duct work Size(Ph)(mm)##other##,Duct work Size(Ph)(inch)##other##,Supply Air Fan Qty (EA)##other##,Supply Air Fan Type##other##,Exhaust Air Fan Qty (EA)##other##,Exhaust Air Fan Type##other##,Filters Qty (EA)##other##,Filters Type##other##,Filters Size (WxHxD)(mm)##other##,Filters Size (WxHxD)(inch)##other##,Type##other##,Chassis name##other##,Model name##other##
ZE080GUCDA0,800,471,"1, 220-240, 50/60",2.2 / 1.4 / 0.8,330 / 200 / 100,800 / 640 / 480,471 / 377 / 283,160 / 102 / 57,77 / 79 / 82,68 / 70 / 73,73 / 76 / 79,-,39 / 34 / 28,59 / 54 / 48,-,-,-,-,-,-,-,54.4,-,1062 x 365 x 1240,-,4,250,-,1,Sirocco fan,1,Sirocco fan,G4:1 / M5:2 + F7:2,OA : G4 / RA : M5+F7,(1156x6x212.5)/(578x25x214),-,ERV,ZC10,ZE080GUCDA0
ZE100GUCDA0,1000,589,"1, 220-240, 50/60",3.0 / 1.9 / 1.0,475 / 280 / 140,1000 / 800 / 600,589 / 471 / 353,160 / 102 / 57,74 / 75 / 77,63 / 67 / 71,72 / 73 / 74,-,40 / 36 / 29,62 / 56 / 52,-,-,-,-,-,-,-,54.4,-,1062 x 365 x 1240,-,4,250,-,1,Sirocco fan,1,Sirocco fan,G4:1 / M5:2 + F7:2,OA : G4 / RA : M5+F7,(1156x6x212.5)/(578x25x214),-,ERV,ZC10,ZE100GUCDA0
