,Normal Capacity (CMH)##other##,Normal Capacity (CFM)##other##,Power Supply (Ph_V_Hz)##other##,ERV Mode Current (SH/H/L)(A)##other##,ERV Mode Power Input (SH/H/L)(W)##other##,ERV Mode Air Flow (SH/H/L)(CMH)##other##,ERV Mode Air Flow (SH/H/L)(CFM)##other##,ERV Mode External static pressure (SH/H/L)(Pa)##other##,ERV Mode Temperature exchange efficiency (SH/H/L)(%)##other##,ERV Mode Enthalpy exchange efficiency Heating (SH/H/L)(%)##other##,ERV Mode Enthalpy exchange efficiency Cooling (SH/H/L)(%)##other##,ERV Mode Energy Label (A+ to G Scale)##other##,ERV Mode Sound pressure level (SH/H/L)(dB(A))##other##,ERV Mode Sound power level (SH/H/L)(dB(A))##other##,Bypass Mode Current (SH/H/L)(A)##other##,Bypass Mode Power Input (SH/H/L)(W)##other##,Bypass Mode Air Flow (SH/H/L)(CMH)##other##,Bypass Mode Air Flow (SH/H/L)(CFM)##other##,Bypass Mode External static pressure (SH/H/L)(Pa)##other##,Bypass Mode Sound pressure level (SH/H/L)(dB(A))##other##,Heat Exchanger type##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Dimensions (WxHxD)(mm)##other##,Dimensions (WxHxD)(inch)##other##,Duct work Qty(EA)##other##,Duct work Size(Ph)(mm)##other##,Duct work Size(Ph)(inch)##other##,Supply Air Fan Qty (EA)##other##,Supply Air Fan Type##other##,Exhaust Air Fan Qty (EA)##other##,Exhaust Air Fan Type##other##,Filters Qty (EA)##other##,Filters Type##other##,Filters Size (WxHxD)(mm)##other##,Filters Size (WxHxD)(inch)##other##,Type##other##,Chassis name##other##,Model name##other##
ZE050GUCCA0,500,294,"1, 220-240, 50/60",1.7 / 1.2 / 0.8,250 / 160 / 105,500 / 400 / 300,294 / 235 / 176,150 / 96 / 54,79 / 79 / 82,68 / 68 / 75,75 / 75 / 78,-,39 / 34 / 29,58 / 56 / 47,-,-,-,-,-,-,-,41.7,-,1014 x 273 x 988,-,4,200,-,1,Sirocco fan,1,Sirocco fan,G4:1 / M5:2 + F7:2,OA : G4 / RA : M5+F7,(855x230x6)/(425x224x25),-,ERV,ZC05,ZE050GUCCA0
