,Circuit Breaker (A)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(mm)##other##,Efficiency (Cooling)##other##,Efficiency (Heating)##other##,Evaporator Flow rate (Cooling)(LPM)##other##,Evaporator Flow rate (Heating)(LPM)##other##,Evaporator Head Loss (kPa)##other##,Evaporator Type##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fin Type##other##,Heating Capacity (kW)##other##,Net Weight (kg)##other##,Operating Current (A)##other##,Piping Connections Inlet (mm)##other##,Piping Connections Outlet (mm)##other##,Power Communication Cable##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling/Heating (dB(A))##other##
"ACHH020LBAB",60,120,Scroll,65,765x2293x2154,2.93,3.25,186,200,21.5,plate,EEV,210x2 @1000rpm,900x2,BLDC,-,70.3,520,39,65A,65A,25.0x5C,22.18430034,21.63076923,"3,380-415,50/60",7.0 kg x 2,R410A,67
"ACHH023LBAB",60,120,Scroll,74,765x2293x2154,2.7,3,211,235,28.7,plate,EEV,210x2 @1000rpm,900x2,BLDC,-,82,520,48,65A,65A,25.0x5C,27.40740741,27.33333333,"3,380-415,50/60",7.0 kg x 2,R410A,68

