,Circuit Breaker (A)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(mm)##other##,Efficiency (Cooling)##other##,Efficiency (Heating)##other##,Evaporator Flow rate (Cooling)(LPM)##other##,Evaporator Flow rate (Heating)(LPM)##other##,Evaporator Head Loss (kPa)##other##,Evaporator Type##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fin Type##other##,Heating Capacity (kW)##other##,Net Weight (kg)##other##,Operating Current (A)##other##,Piping Connections Inlet (mm)##other##,Piping Connections Outlet (mm)##other##,Power Communication Cable##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling/Heating (dB(A))##other##
"ACHH050LBAB",200,60x6,Scroll,171,2291x2293x2154,3.1,3.4,490,518,18.7,plate,EEV,210x6 @1000rpm,900x6,BLDC,-,180,1430,108,65A,65A,95.0x5C,55.16129032,52.94117647,"3,380-415,50/60",7.0 kg x 6,R410A,68
"ACHH060LBAB",200,60x6,Scroll,195,2291x2293x2154,2.93,3.25,558,600,21.5,plate,EEV,210x6 @1000rpm,900x6,BLDC,-,210.9,1430,117,65A,65A,95.0x5C,66.55290102,64.89230769,"3,380-415,50/60",7.0 kg x 6,R410A,68
"ACHH067LBAB",200,60x6,Scroll,222,2291x2293x2154,2.7,3,633,705,28.7,plate,EEV,210x6 @1000rpm,900x6,BLDC,-,246,1430,144,65A,65A,95.0x5C,82.22222222,82,"3,380-415,50/60",7.0 kg x 6,R410A,68

