,Circuit Breaker (A)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(mm)##other##,Efficiency (Cooling)##other##,Efficiency (Heating)##other##,Evaporator Flow rate (Cooling)(LPM)##other##,Evaporator Flow rate (Heating)(LPM)##other##,Evaporator Head Loss (kPa)##other##,Evaporator Type##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fin Type##other##,Heating Capacity (kW)##other##,Net Weight (kg)##other##,Operating Current (A)##other##,Piping Connections Inlet (mm)##other##,Piping Connections Outlet (mm)##other##,Power Communication Cable##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling/Heating (dB(A))##other##
"ACHH040LBAA",125,60x4,Scroll,123,1528x2351x2154,2.65,3.2,353,404,34,Plate,Electronic Expansion Valve,210x4@1000rpm,900x4,BLDC,Wide Louver,141.0,1030,104,65A,65A,50.0x5C,46.4,43.9,"3,380-415,50/60",14x2,R410A,68
"ACAH040LBAA",125,60x4,Scroll,123,1528x2351x2154,2.65,-,353,-,34,Plate,Electronic Expansion Valve,210x4@1000rpm,900x4,BLDC,Wide Louver,-,1030,104,65A,65A,50.0x5C,46.4,-,"3,380-415,50/60",15x2,R410A,68

