,Circuit Breaker (A)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(mm)##other##,Efficiency (Cooling)##other##,Efficiency (Heating)##other##,Evaporator Flow rate (Cooling)(LPM)##other##,Evaporator Flow rate (Heating)(LPM)##other##,Evaporator Head Loss (kPa)##other##,Evaporator Type##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fin Type##other##,Heating Capacity (kW)##other##,Net Weight (kg)##other##,Operating Current (A)##other##,Piping Connections Inlet (mm)##other##,Piping Connections Outlet (mm)##other##,Power Communication Cable##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling/Heating (dB(A))##other##
"ACHH033LBAB",125,60x4,Scroll,114,1528x2293x2154,3.1,3.4,327,345,18.7,plate,EEV,210x4 @1000rpm,900x4,BLDC,-,120,970,72,65A,65A,50.0x5C ,36.77419355,35.29411765,"3,380-415,50/60",7.0 kg x 4,R410A,68
"ACHH040LBAB",125,60x4,Scroll,130,1528x2293x2154,2.93,3.25,372,400,21.5,plate,EEV,210x4 @1000rpm,900x4,BLDC,-,140.6,970,78,65A,65A,50.0x5C ,44.36860068,43.26153846,"3,380-415,50/60",7.0 kg x 4,R410A,68
"ACHH045LBAB",125,60x4,Scroll,148,1528x2293x2154,2.7,3,411,470,28.7,plate,EEV,210x4 @1000rpm,900x4,BLDC,-,164,970,96,65A,65A,50.0x5C ,54.81481481,54.66666667,"3,380-415,50/60",7.0 kg x 4,R410A,68

