,Circuit Breaker (A)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(mm)##other##,Efficiency (Cooling)##other##,Efficiency (Heating)##other##,Evaporator Flow rate (Cooling)(LPM)##other##,Evaporator Flow rate (Heating)(LPM)##other##,Evaporator Head Loss (kPa)##other##,Evaporator Type##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fin Type##other##,Heating Capacity (kW)##other##,Net Weight (kg)##other##,Operating Current (A)##other##,Piping Connections Inlet (mm)##other##,Piping Connections Outlet (mm)##other##,Power Communication Cable##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling/Heating (dB(A))##other##
"ACHH060LBAA",200,60x6,Scroll,185,2291 x 2351 x 2154,2.65,3.2,531,604,34,Plate,Electronic Expansion Valve,210x6@1000rpm,900x6,BLDC,Wide Louver,211,1530,156,65A,65A,95.0x5C,69.8,65.9,"3,380-415,50/60",14x3,R410A,68
"ACAH060LBAA",200,60x6,Scroll,185,2291 x 2351 x 2154,2.65,-,531,-,34,Plate,Electronic Expansion Valve,210x6@1000rpm,900x6,BLDC,Wide Louver,211,1530,156,65A,65A,95.0x5C,69.8,-,"3,380-415,50/60",15x3,R410A,68

