,Circuit Breaker (A)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(mm)##other##,Efficiency (Cooling)##other##,Efficiency (Heating)##other##,Evaporator Flow rate (Cooling)(LPM)##other##,Evaporator Flow rate (Heating)(LPM)##other##,Evaporator Head Loss (kPa)##other##,Evaporator Type##other##,Expansion Valve Type##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (W)##other##,Fan Motor Type##other##,Fin Type##other##,Heating Capacity (kW)##other##,Net Weight (kg)##other##,Operating Current (A)##other##,Piping Connections Inlet (mm)##other##,Piping Connections Outlet (mm)##other##,Power Communication Cable##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling/Heating (dB(A))##other##
"ACHH020LBAA",75,60x2,Scroll,60,765x2351x2154,2.63,3.2,172,202,58.2,Plate,Electronic Expansion Valve,210x2@1000rpm,900x2,BLDC,Wide Louver,70.3,540,52,40A,40A,25.0x5C,22.8,22.0,"3,380-415,50/60",14x1,R410A,67
"ACAH020LBAA",75,60x2,Scroll,60,765x2351x2154,2.63,-,172,-,58.2,Plate,Electronic Expansion Valve,210x2@1000rpm,900x2,BLDC,Wide Louver,-,540,52,40A,40A,25.0x5C,22.8,-,"3,380-415,50/60",15x1,R410A,67

