,Compressor Motor Output (kW)##other##,Compressor Type##other##,Drain Outlet Diameter1##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kcal/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(mm)##other##,Free Contents Download##other##,Heat Exchanger Head Loss (kPa)##other##,Heat Exchanger Maximum Pressure Resistance (kg/cm2)##other##,Heat Exchanger Rated Water Flow (LPM)##other##,Heat Exchanger Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kcal/h)##other##,Heating Capacity (kW)##other##,Independent Unit##other##,Indoor Unit Model Max Quantity##other##,Indoor Unit Total Capacity##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_High Gas Side (inch)##other##,Pipe Connection_High Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Pipe Connection_Low Gas Side (inch)##other##,Pipe Connection_Low Gas Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,"Power Supply (Ph,V,Hz)"##other##,Refrigerant Charge (Kg)##other##,High Gas Pipe Diameter1##other##,Liquid Pipe Diameter1##other##,Low Gas Pipe Diameter1##other##,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Heating)(C)##other##,Transmission Cable##other##,Type##other##,Water Inlet Pipe Diameter1##other##,Water Outlet Pipe Diameter1##other##
"ARWB80LAS4",4.2, Hermetically Sealed Scroll  ,20,76400,19300,22.4,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,36.5,45,77,Stainless Steel Plate,86000,21700,25.2,ARWB80LAS4,13(20),50% to 130% of Outdoor Unit Capacity,24,ARWB80LAS4,120 x 1,20,3/4,19.05,3/8,9.52,7/8,22.2,3.86,4.2,"3 ,380-415,50/3,380,60",5.5,19.05,9.52,22.2,R410A,47,51,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV Heat Recovery,40,40
"ARWB100LAS4",4.2, Hermetically Sealed Scroll  ,20,95500,24100,28,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,36.5,45,96,Stainless Steel Plate,107500,27100,31.5,ARWB100LAS4,16(25),50% to 130% of Outdoor Unit Capacity,24.5,ARWB100LAS4,120 x 1,20,3/4,19.05,3/8,9.52,7/8,22.2,5.09,5.34,"3 ,380-415,50/3,380,60",5.5,19.05,9.52,22.2,R410A,50,53,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV Heat Recovery,40,40
"ARWB120LAS4",4.2, Hermetically Sealed Scroll  ,20,114600,28900,33.6,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,36.5,45,116,Stainless Steel Plate,129000,32500,37.8,ARWB120LAS4,20(30),50% to 130% of Outdoor Unit Capacity,25,ARWB120LAS4,120 x 1,20,3/4,19.05,1/2,12.7,7/8,22.2,6.46,6.75,"3 ,380-415,50/3,380,60",5.5,19.05,12.7,22.2,R410A,56,56,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV Heat Recovery,40,40
"ARWB140LAS4",4.2, Hermetically Sealed Scroll  ,20,133800,33700,39.2,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,36.5,45,135,Stainless Steel Plate,150500,37900,44.1,ARWB140LAS4,23(35),50% to 130% of Outdoor Unit Capacity,25.5,ARWB140LAS4,120 x 1,20,3/4,19.05,1/2,12.7,1,25.4,7.84,8.17,"3 ,380-415,50/3,380,60",5.5,19.05,12.7,25.4,R410A,58,57,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV Heat Recovery,40,40
"ARWB160LAS4",5.3, Hermetically Sealed Scroll  ,20,152900,38500,44.8,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,31.8,45,154,Stainless Steel Plate,172000,43300,50.4,ARWB160LAS4,26(40),50% to 130% of Outdoor Unit Capacity,32,ARWB160LAS4,140 x 1,20,3/4,19.05,1/2,12.7,1-1/8,28.58,8.15,8.54,"3 ,380-415,50/3,380,60",6.6,19.05,12.7,28.58,R410A,53,57,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV Heat Recovery,40,40
"ARWB180LAS4",5.3, Hermetically Sealed Scroll  ,20,172000,43300,50.4,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,31.8,45,173,Stainless Steel Plate,193500,48800,56.7,ARWB180LAS4,29(45),50% to 130% of Outdoor Unit Capacity,32.5,ARWB180LAS4,140 x 1,20,3/4,19.05,1/2,12.7,1-1/8,28.58,9.69,10.13,"3 ,380-415,50/3,380,60",6.6,19.05,12.7,28.58,R410A,55,56,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV Heat Recovery,40,40
"ARWB200LAS4",5.3,Hermetically Sealed Scroll,20,191100,48200,56,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,31.8,45,192,Stainless Steel Plate,215000,54200,63,ARWB200LAS4,32(44),50% to 130% of Outdoor Unit Capacity,33,ARWB200LAS4,140 x 1,20,3/4,19.05,1/2,12.7,1-1/8,28.58,11.2,11.67,"3 ,380-415,50/3,380,60",6.6,19.05,12.7,28.58,R410A,54,60,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV Heat Recovery,40,40

